**PK Ranger**

|  |  |
| --- | --- |
| Lowcut Available | No |
| Available Vehicle Models | Ford Ranger PK |
| Custom airbox Available | No |
| Is the snorkel recessed? | Yes |
| How does the snorkel mount? | Rivets through the bracket into the pillar and a small tab through the back of the guard. Line the snorkel up first then mark where the bracket holes sit on your pillar and rivet the bracket in pace before installing the snorkel. |
| Available finishes | Polished, powder coated or painted |
| Will it cover pre-existing snorkel? | No |
| Will it plumb to standard airbox? | Yes |
| Installation kit | Polyurethane pipe, rubber pinchweld, hose clamps, cut out template and pop rivets |
| Material used | 4” 316 marine grade stainless steel |
| Seamless welds | Yes |
| Noise | Loud with a pod filter, quiet with a panel filter |
| Install difficulty (1-10) | 3 |
| Tools Required | Tin snips, drill, rivet gun, spanners/sockets, screwdrivers, |
| Will it work with a dual battery setup? | Yes |
| Price of snorkel | $850 + GST |
| Postage Insurance | $50 for a snorkel, $30 for an airbox and $80 for the combo |
| Time until delivery | 4-5 Weeks or 1 week express ($300 + GST) |
| When will the snorkel be on the way? | You will receive a tracking number on the day your order leaves the factory. |
| Is this snorkel in stock? | No, all snorkels are made to order |