**Ranger Raptor Combo**

|  |  |
| --- | --- |
| Lowcut Available | No |
| Available Vehicle Models | Ranger Raptor |
| Custom airbox Available | The raptor is a combo only product as the snorkel will not plumb to the factory airbox |
| Is the snorkel recessed? | Yes |
| How does the snorkel mount? | Rivets through the bracket into the pillar and a small tab through the back of the guard |
| Available finishes | Polished, powder coated or painted |
| Will it plumb to standard airbox? | No |
| Installation kit | 3 ½” Polyurethane pipe, rubber pinchweld, 2x hose clamps, cut out template and pop rivets |
| Material used | 4” 316 marine grade stainless steel |
| Seamless welds | Yes |
| Install difficulty (1-10) | 5 |
| Connecting snorkel to airbox | You will need to cut a hole through the inside engine bay wall big enough to fir the flexi pipe through. Apply pinch weld around sharp edges. |
| Air filters used | K&N Pod Filters |
| Cleaning filters | Use filter cleaning kit when dirty |
| Intake Pipe | Not included but available |
| Tools Required | Hack saw, drill, rivet gun, spanners/sockets, screwdrivers, |
| Will it work with a dual battery setup? | Yes |
| Price for combo | $1400 + GST |
| Postage Insurance | $50 for a snorkel, $30 for an airbox and $80 for the combo |
| Time until delivery | 4-5 Weeks or 1 week express ($300 + GST) |
| When will the snorkel be on the way? | You will receive a tracking number on the day your order leaves the factory. |
| Is this snorkel in stock? | No, all snorkels are made to order |